[1. Introduction 2](#_Toc417841415)

[1.1. Purpose 2](#_Toc417841416)

[1.2. Intended Audience and Reading Suggestions 2](#_Toc417841417)

[1.3. Scope 2](#_Toc417841418)

[1.3.1. Mandated Time Constraints 3](#_Toc417841419)

[1.4. Outstanding Issues 3](#_Toc417841420)

[1.5. References 3](#_Toc417841421)

[2. Assumptions 4](#_Toc417841422)

[3. System Features 4](#_Toc417841423)

[3.1. Fire extinguishing system 4](#_Toc417841424)

[3.1.1. General description 4](#_Toc417841425)

[3.1.2. Use cases 4](#_Toc417841426)

[3.2. Door security system 7](#_Toc417841427)

[3.2.1. General description 7](#_Toc417841428)

[3.2.2. Use cases 7](#_Toc417841429)

[3.3 Garage security system 8](#_Toc417841430)

[3.3.1. General description 8](#_Toc417841431)

[3.3.2. Use cases 8](#_Toc417841432)

[3.4 Window security system 10](#_Toc417841433)

[3.4.1. General description 10](#_Toc417841434)

[3.4.2. Use cases 10](#_Toc417841435)

[3.5 CCTV system 11](#_Toc417841436)

[3.5.1. General description 11](#_Toc417841437)

[3.5.2. Use cases 11](#_Toc417841438)

[3.6 Web-based monitoring dashboard system 13](#_Toc417841439)

[3.6.1. General description 13](#_Toc417841440)

[3.6.2. Use cases 13](#_Toc417841441)

[4. Non-functional Requirements 15](#_Toc417841442)

[4.1. Performance Requirements 15](#_Toc417841443)

[4.1.1. Network Performance Requirements 15](#_Toc417841444)

[4.1.2. Storage Requirements 15](#_Toc417841445)

[4.1.3. Memory/Architecture Requirements 15](#_Toc417841446)

[4.1.4. Design/Physical Factor Requirements 15](#_Toc417841447)

[4.2. Process Requirements 16](#_Toc417841448)

[4.2.1. Standard Requirements 16](#_Toc417841449)

[4.2.2. Management Requirements 16](#_Toc417841450)

[4.3. Software Quality Requirements 17](#_Toc417841451)

[4.4. Security Requirements 17](#_Toc417841452)

[4.4.1. Access Permission 17](#_Toc417841453)

[4.4.2. Privacy 17](#_Toc417841454)

[APPENDIX 18](#_Toc417841455)

[A. Change Log 18](#_Toc417841456)

[B. Glossary 18](#_Toc417841457)

[C. Authorship 18](#_Toc417841458)

# Introduction

## Purpose

The purpose of this SRS document is to provide the functional requirements and other non-functional requirements for the SafeHome project, the final project of their CS350 course, carried out by team 2 members (consisting Young Seok Kim and Seokju Hong).

## Intended Audience and Reading Suggestions

Main reader of this document is supposed to be CS350 team 2 members, Young Seok Kim and Seokju Hong, who will implement the whole component of SafeHome. This document is written to help understand whole project clearly, reduce the gap between each other’s ideas on the project, and encourage collaboration. Another target reader of this document is teaching assistants and professor of CS350, which is held in 2015 spring semester, to evaluate team 2’s work on SRS.

Followings are the brief summaries of each chapter.

1. “Chapter 1: Introduction” provides overview of the SafeHome project: the goal of the project, purpose of this document, scope of this project, outstanding issues, and references.
2. “Chapter 2: Assumptions” provides assumptions used over the SafeHome project design.
3. “Chapter 3: System features” provides brief summary of to-be-implemented features of the SafeHome project, analysis on assumptions, constraints, use-cases, and acceptance criteria of each features.
4. “Chapter 4: Non-functional requirements” provides any requirements other than functional requirements, such as performance requirements, process requirements, quality requirements, and security requirements.
5. Change log, Glossary, Authorship table and any other information that is needed to understand whole document will be written on appendixes.

## Scope

The goal of this project is to implement home security and surveillance system and software “SafeHome” in an innovative tiny box. Members of team 2 are expected to write documents, make analyze models, and implement the SafeHome project.

The system is expected to serve many features and functions to alarm and prevent possible risks and accidents, such as fire over the house, or any other safety issues or accidents. For example, for fire incident over house, sensors like carbon monoxide sensor or temperature sensor will measure the environment of the house and if SafeHome system decides that fire incident happens in the house, it will alarm whole house, call 119, and send messages to registered contact.

The system also serves as a surveillance system. To prevent robbery or trespass of strangers, this system includes observation system based on CCTV. If unidentified person approaches the house and tries to enter the house, the system will alarm over the house, call 112, and send messages to registered contacts. Also, it will try to manipulate the door lock components to secure properties of household.

This system also serves web-based dashboards and API’s to let user observe status of the house and control security system of the SafeHome box. A user may want to look over his or her home and see whether things are in good state. Some user may not want to use specific features because of any reasons. To cover those overview/manipulation use cases, the SafeHome project basically serves web-based dashboards. And for more improvements on interfaces, it will also provide API of the dashboard app.

There are many features and functions that will be implemented at the version 1.0, however, as this is a software project, it will evolve. More possible risk-preventing features and improvements are expected to be implemented in the software product line.

### Mandated Time Constraints

Phase I: Write SRS documents (by Apr. 26)

Phase II: Design analysis model (TBA)

Phase III: Construct design model (TBA)

Phase IV: Construct and deploy project (TBA)

## Outstanding Issues

None to date (Refer to the last updated date)

## References

*"Google Java Style." Google Java Style. Google, 21 Mar. 2014. Web. 26 Apr. 2015.*

*Kim, Monzoo. "CS350 Intro. to SE Spring 15." — SW Testing & Verification Group. KAIST, n.d. Web. 26 Apr. 2015.*

*Rojas, Francisco, et al, “SRS for SafeHome System”, March 11, 2009*

*Choi, Jinho, “Software Requirements Specification for SafeHome Project”, Mar 11th 2009*

*Hong, Chanki, “Safehome Project Requirements Specification”, March 11, 2009*

*Pressman, Roger S. Software Engineering: A Practitioner's Approach 8th edition. N.p.: n.p., n.d. Print.*

# Assumptions

The following are assumptions made in this design:

1. SafeHome box is connected to the internet.
2. SafeHome is expected to update via internet when some security patches are available.
3. Operating temperature of the device is expected to be from -10 degree Celsius to 50 degree Celsius.
4. SafeHome is expected to be connected to the power outlet properly.
5. SafeHome is expected to run 1~2 days even after power outage happens.
6. SafeHome uses safe encrypted communication and if related security issues happen, related patches will be automatically applied.
7. SafeHome console is expected to be durable even with free falling with 2 meter height.
8. Assumes critical sensor error happens rarely: monthly sensor check service will be held and broken sensors are changed as soon as possible.

# System Features

## Safehome bootup/shutdown service

### General description

This feature is needed in order to boot up the main safehome system and do shut down. In order to use many of the features, the bootup is required in order to use those services

### Use cases

* + - 1. Bootup

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.1.2.1 | Feature Number | 3.1 | Frequency of Use | Rarely |
| Created date | 6/5/2015 | Author | Young Seok Kim | Owner | Young Seok Kim |
| Updated date | 6/5/2015 | Updated by | Young Seok Kim | Revision # | 0 |
| Priority | High | | | | |
| Primary actor | SafeHome system, User | | | | |
| Title | Bootup | | | | |
| Preconditions | SafeHome system is shut down | | | | |
| Postconditions | SafeHome system is booted up | | | | |
| Main success scenario | 1. User press the power button. 2. SafeHome system boots up. | | | | |
| Exceptions | 1a. SafeHome system is not connected to the power source. | | | | |

* + - 1. Shut down

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.1.2.2 | Feature Number | 3.1 | Frequency of Use | Rarely |
| Created date | 6/5/2015 | Author | Young Seok Kim | Owner | Young Seok Kim |
| Updated date | 6/5/2015 | Updated by | Young Seok Kim | Revision # | 0 |
| Priority | High | | | | |
| Primary actor | SafeHome system, User | | | | |
| Title | Shutdown | | | | |
| Preconditions | SafeHome system is booted up | | | | |
| Postconditions | SafeHome system is shut down | | | | |
| Main success scenario | 1. User press the power button. 2. SafeHome system boots up. | | | | |
| Exceptions |  | | | | |

## Configuration service

### General description

Originally, this service configures the user password, floor plan, security zone, and session timeout. The scope of the project was reduced to password and security zone.

### Use cases

* + - 1. Password configuration

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.2.2.1 | Feature Number | 2 | Frequency of Use | Rare, first time only |
| Created date | 5/4/2015 | Author | Young Seok Kim | | |
| Updated date | 6/5/2015 | Updated by | Young Seok Kim | Revision # | 2 |
| Priority | High | | | | |
| Primary actor | SafeHome system, User | | | | |
| Title | Password Registration – Control panel | | | | |
| Preconditions | SafeHome system password is not set | | | | |
| Trigger | User first boots up SafeHome system | | | | |
| Postconditions | SafeHome system password setting is finished | | | | |
| Main success scenario | 1. User first boots up SafeHome system. 2. Password registration screen shows up. 3. User enters valid password and presses ‘done’ button 4. The password is registered to SafeHome system | | | | |
| Exceptions | 3a. User enters invalid password (must be 4 digits)   * 3a1. SafeHome system shows error message – “invalid password” and asks the user to enter password again. | | | | |

* + - 1. Security zone

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.2.2.2. | Feature Number | 2 | Frequency of Use | Rare |
| Created date | 5/4/2015 | Author | Young Seok Kim | | |
| Updated date | 6/5/2015 | Updated by | Young Seok Kim | Revision # | 2 |
| Priority | Medium | | | | |
| Primary actor | SafeHome system, User, devices | | | | |
| Title | Grouping devices | | | | |
| Preconditions | Devices are properly installed to SafeHome system | | | | |
| Trigger | User accesses grouping device screen on SafeHome system | | | | |
| Postconditions | SafeHome devices are grouped together to be manipulated as groups | | | | |
| Main success scenario | 1. User access grouping device screen on SafeHome system 2. User selects 1 or more devices and presses ‘done’ button 3. Selected devices are registered as groups | | | | |
| Exceptions | 2a. User didn’t select any device and press enter   * 2a1. SafeHome system shows error message – “empty group” and asks the user to select devices again. | | | | |

## Real time security service

### General description

This real time security service includes arming and disarming the system, sensors, and cameras. SafeHome system

### Use cases

## System reporting service

### General description

### Use cases

## Fire extinguishing system

### General description

When fire accident happens, or some factors that can cause fire are detected by the SafeHome system’s sensors, the SafeHome system have to deal with those cases. For example, suppose someone turned on gas burner and did not turned off for a long time. The SafeHome box have to detect it with its gas sensor, and turn it off. Or, for the another case, if a fire break out at the house, the SafeHome system have to activate spring cooler and any other possible actuators to cease fires, and help people in the house to escape from the house. Like these examples, fire extinguishing system component serves features related to fire breaking out: helping evacuation, ceasing fire, and any possible actions that it can perform.

### Use cases

#### Gas leak alert

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.1.2.1 | Feature Number | 3.1 | Frequency of Use | Rarely |
| Created date | 4/25/2015 | Author | Seokju Hong | Owner | Seokju Hong |
| Updated date | 4/25/2015 | Updated by | Seokju Hong | Revision # | 0 |
| Priority | Medium | | | | |
| Primary actor | SafeHome system, User | | | | |
| Title | Gas leak alert | | | | |
| Preconditions | User has set the configuration to use “Gas leak alert”  Gas leaks from LPG hose and SafeHome sensor detects high level of LPG gas | | | | |
| Postconditions | Gas leak stop and ppm of LPG gas is lower than threshold value. | | | | |
| Main success scenario | 1. SafeHome system records log to SafeHome dashboard system and set status value as “Warning” 2. SafeHome actuator tries to control valve to lower the concentration of LPG. 3. LPG concentration decreases, and ppm value is lower than threshold value. 4. SafeHome system records log to SafeHome dashboard system and set status value as “OK” | | | | |
| Exceptions | 1a. SafeHome gas sensor didn’t detected high level of LPG gas  3a. SafeHome fails to lower the concentration of LPG for 5 minutes(timeout)   * 2a1. The SafeHome system sends message to registered contact that lowering gas level failed. * 2a2. The SafeHome system powers ventilating system on to lower gas level. | | | | |

#### Fire alert

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.1.2.2 | Feature Number | 3.1 | Frequency of Use | Rarely |
| Created date | 4/25/2015 | Author | Seokju Hong | Owner | Seokju Hong |
| Updated date | 4/25/2015 | Updated by | Seokju Hong | Revision # | 0 |
| Priority | High | | | | |
| Primary actor | SafeHome system | | | | |
| Title | Fire alert | | | | |
| Preconditions | User has set configuration to use “Fire alert”  Carbon monoxide concentration value is over threshold value, and temperature value is over threshold value | | | | |
| Postconditions |  | | | | |
| Main success scenario | 1. Carbon monoxide concentration value and temperature, which measured from the SafeHome sensors, are over its threshold value. 2. The SafeHome system sends message to 119, and registered contract. 3. The SafeHome system triggers siren over the house. 4. The SafeHome system calls registered callbacks related with the fire alarm system(e.g. use case 3.1.2.3.) and initiate emergency features. | | | | |
| Exceptions | 2a. No registered contact on SafeHome system   * 2a1. The SafeHome system doesn’t send messages. | | | | |

#### Evacuation guide

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.1.2.3 | Feature Number | 3.1 | Frequency of Use | Rarely |
| Created date | 4/25/2015 | Author | Seokju Hong | Owner | Seokju Hong |
| Updated date | 4/25/2015 | Updated by | Seokju Hong | Revision # | 0 |
| Priority | High | | | | |
| Primary actor | SafeHome system, People in the house | | | | |
| Title | Evacuation guide | | | | |
| Preconditions | Fire alert function called. | | | | |
| Postconditions |  | | | | |
| Main success scenario | 1. Evacuation guide feature works as soon as the fire alert function called. 2. For every door in the house, the SafeHome system evaluates safety level and select doors safe enough to escape. 3. Turn every evacuation guide lamp on that leads to the door selected at step 2. 4. Every people in the house follows the lamp and succeeds to escape. | | | | |
| Exceptions | 2a. There’s no available safe door.   * 2a1. The SafeHome system evaluates safety level for windows. If there are any safe windows, turn every evacuation guide lamp that leads to the window selected on evaluation step * 2a2. If SafeHome still fails to find safe out, retry evaluation after 3 minutes. | | | | |

#### Spring cooler activation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.1.2.4 | Feature Number | 3.1 | Frequency of Use | Rarely |
| Created date | 4/25/2015 | Author | Seokju Hong | Owner | Seokju Hong |
| Updated date | 4/25/2015 | Updated by | Seokju Hong | Revision # | 0 |
| Priority | High | | | | |
| Primary actor | SafeHome system | | | | |
| Title | Spring cooler activation | | | | |
| Preconditions | Fire alert function called | | | | |
| Postconditions |  | | | | |
| Main success scenario | 1. Spring cooler activation function called 2. Activates every spring cooler in the house | | | | |
| Exceptions |  | | | | |

## Door security system

### General description

SafeHome system provides door security system. Door security system notifies the users if door is unlocked for a long time. The users can also lock or unlock the door with the button. In addition, the users can monitor if the door is locked or unlocked. For example, if the user forgot to lock the door and leave the door open for 20 minutes, then SafeHome device will notify the user that the door is opened. Then, the user can lock the door with the SafeHome device. In addition, if someone visited the house and rang the doorbell, then the user can unlock the door with the SafeHome device.

### Use cases

#### Unlocked door notification

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.2.2.1 | Feature Number | 3.2 | Frequency of Use | Sometimes |
| Created date | 4/25/2015 | Author | Young Seok Kim | Owner | Young Seok Kim |
| Updated date | 4/25/2015 | Updated by | Young Seok Kim | Revision # | 0 |
| Priority | High | | | | |
| Primary actor | SafeHome system, user, door | | | | |
| Title | Unlocked door notification | | | | |
| Preconditions | Door security system is activated.  The door is opened for more than 20 minutes. | | | | |
| Postconditions | The door notification is turned on. | | | | |
| Main success scenario | 1. User unlocks the door. 2. SafeHome system is notified and waits for 20minutes 3. SafeHome system alerts the user that the door is opened | | | | |
| Exceptions |  | | | | |

#### Lock door

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.2.2.2 | Feature Number | 3.2 | Frequency of Use | Sometimes |
| Created date | 4/25/2015 | Author | Young Seok Kim | Owner | Young Seok Kim |
| Updated date | 4/25/2015 | Updated by | Young Seok Kim | Revision # | 0 |
| Priority | High | | | | |
| Primary actor | SafeHome system, user, door | | | | |
| Title | Lock door | | | | |
| Preconditions | Door security system is activated.  The door is currently unlocked | | | | |
| Postconditions | The door gets locked | | | | |
| Main success scenario | 1. User presses lock button in SafeHome system 2. The door gets locked. | | | | |
| Exceptions | 2a. The door is already locked   * 2a1. SafeHome notifies the user that the door is already locked. | | | | |

#### Unlock door

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.2.2.3 | Feature Number | 3.2 | Frequency of Use | Sometimes |
| Created date | 4/25/2015 | Author | Young Seok Kim | Owner | Young Seok Kim |
| Updated date | 4/25/2015 | Updated by | Young Seok Kim | Revision # | 0 |
| Priority | High | | | | |
| Primary actor | SafeHome system, user, door | | | | |
| Title | Lock door | | | | |
| Preconditions | Door security system is activated.  The door is currently locked | | | | |
| Postconditions | The door gets unlocked | | | | |
| Main success scenario | 1. User presses unlock button in SafeHome system 2. The door gets unlocked. | | | | |
| Exceptions | 2a. The door is already unlocked   * 2a1. SafeHome notifies the user that the door is already unlocked. | | | | |

## Garage security system

### 3.3.1. General description

SafeHome also secure the garage of the user. The garage security system notifies if the garage door is opened. Also, the user can open/close the garage door by the SafeHome system. For example, if the user forgot to close the garage door, the SafeHome garage security system notifies the user. In addition, if someone visits the user’s house, the user can open the garage, or close the garage.

### 3.3.2. Use cases

#### 3.3.2.1. Opened garage door notification

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.3.2.1 | Feature Number | 3.3 | Frequency of Use | Often |
| Created date | 4/25/2015 | Author | Young Seok Kim | Owner | Young Seok Kim |
| Updated date | 4/25/2015 | Updated by | Young Seok Kim | Revision # | 0 |
| Priority | High | | | | |
| Primary actor | SafeHome system, user, garage door | | | | |
| Title | Opened garage door notification | | | | |
| Preconditions | Garage security system is activated.  The garage door is currently opened for 20 minutes. | | | | |
| Postconditions | Opened garage door notification is turned on. | | | | |
| Main success  scenario | 1. The garage door is opened. 2. SafeHome waits for 20 minutes. 3. SafeHome alerts the user that the garage door is opened. | | | | |
| Exceptions | 2a. The door is already unlocked   * 2a1. SafeHome notifies the user that the door is already unlocked. | | | | |

#### 3.3.2.2. Opening garage door

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.3.2.2 | Feature Number | 3.3 | Frequency of Use | Often |
| Created date | 4/25/2015 | Author | Young Seok Kim | Owner | Young Seok Kim |
| Updated date | 4/25/2015 | Updated by | Young Seok Kim | Revision # | 0 |
| Priority | High | | | | |
| Primary actor | SafeHome system, user, garage door | | | | |
| Title | Opening garage door | | | | |
| Preconditions | Garage security system is activated.  The garage door is currently closed | | | | |
| Postconditions | The garage door is opened | | | | |
| Main success  scenario | 1. The user presses “open garage door” button. 2. SafeHome device opens the garage door. | | | | |
| Exceptions | 2a. The garage door is already opened.   * 2a1. SafeHome notifies the user that the garage door is already opened. | | | | |

#### 3.3.2.3. Closing garage door

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.3.2.3 | Feature Number | 3.3 | Frequency of Use | Often |
| Created date | 4/25/2015 | Author | Young Seok Kim | Owner | Young Seok Kim |
| Updated date | 4/25/2015 | Updated by | Young Seok Kim | Revision # | 0 |
| Priority | High | | | | |
| Primary actor | SafeHome system, user, garage door | | | | |
| Title | Closing garage door | | | | |
| Preconditions | Garage security system is activated.  The garage door is currently opened. | | | | |
| Postconditions | The garage door is closed. | | | | |
| Main success  scenario | 1. The user presses “close garage door” button. 2. SafeHome device closes the garage door. | | | | |
| Exceptions | 2a. The garage door is already closed   * 2a1. SafeHome notifies the user that the garage door is already closed. | | | | |

## Window security system

### 3.4.1. General description

SafeHome secures the windows of the user’s house. For example, if the window is broken, the sensor is activated and notifies the user immediately. Also, the users can monitor which window is opened and which window is closed by just watching the panel of the SafeHome device.

### 3.4.2. Use cases

#### 3.4.2.1. Broken window notification

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.4.2.1 | Feature Number | 3.4 | Frequency of Use | Rare |
| Created date | 4/25/2015 | Author | Young Seok Kim | Owner | Young Seok Kim |
| Updated date | 4/25/2015 | Updated by | Young Seok Kim | Revision # | 0 |
| Priority | High | | | | |
| Primary actor | SafeHome system, user, window | | | | |
| Title | Broken window notification | | | | |
| Preconditions | Window security system is activated.  The window broken sensor is activated. | | | | |
| Postconditions | The broken window notification is turned on. | | | | |
| Main success  scenario | 1. The window broken sensor is activated. 2. SafeHome device receives the sensor signal. 3. SafeHome device alerts the user that the window is broken. | | | | |
| Exceptions | 1a. The window broken sensor malfunctions   * The user can contact the company to get a replacement for the malfunctioning window broken sensor. | | | | |

#### 3.4.2.2. Window panel

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.4.2.2 | Feature Number | 3.4 | Frequency of Use | Sometimes |
| Created date | 4/25/2015 | Author | Young Seok Kim | Owner | Young Seok Kim |
| Updated date | 4/25/2015 | Updated by | Young Seok Kim | Revision # | 0 |
| Priority | High | | | | |
| Primary actor | SafeHome system, user, window | | | | |
| Title | Window panel | | | | |
| Preconditions | Window security system is activated.  The window openness sensor is functioning well. | | | | |
| Postconditions |  | | | | |
| Main success  scenario | 1. All of the windows in the user’s house gives the openness signal to the SafeHome device. 2. The SafeHome device shows which window is opened and which window is closed | | | | |
| Exceptions | 1a. The window openness sensor malfunctions   * The user can contact the company to get a replacement for the malfunctioning window openness sensor. | | | | |

## CCTV system

### 3.5.1. General description

The SafeHome system provides not only security system, but also surveillance system. The SafeHome security system may send message to registered contact in some cases. But, it can be false-positive as sensor value is not always true. Or, users of the SafeHome system may want to check out if their home is in nice state or not when they got messages. And the robbery case, for example, it need to take a shot of the room to make evidences. Therefore, the SafeHome system includes CCTV-based surveillance system.

### 3.5.2. Use cases

#### Add new CCTV

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.5.2.1 | Feature Number | 3.5 | Frequency of Use | Rarely |
| Created date | 4/25/2015 | Author | Seokju Hong | Owner | Seokju Hong |
| Updated date | 4/25/2015 | Updated by | Seokju Hong | Revision # | 0 |
| Priority | High | | | | |
| Primary actor | SafeHome system, user, CCTV | | | | |
| Title | Add new CCTV | | | | |
| Preconditions | CCTV surveillance system is activated.  New CCTV is compatible with the SafeHome system. | | | | |
| Postconditions | New CCTV added to surveillance system. | | | | |
| Main success scenario | 1. User connects CCTV with the SafeHome console. 2. SafeHome system detects new CCTV 3. SafeHome system sends “Hello” message to CCTV. 4. CCTV responds with “OK” to SafeHome system. 5. SafeHome system registers new CCTV and create related database schema. | | | | |
| Exceptions | 2a. CCTV not detected   * 2a1. User tries to reconnect CCTV   4a. “Hello” message from the SafeHome box corrupted   * 4a1. CCTV send “RECONNECT” message to the SafeHome box * 4a2. If it fails for 3 times, the red LED of the CCTV blinks   4b. The SafeHome system did not received OK, or the message from CCTV corrupted   * 4b1. The SafeHome system resends “Hello” message to CCTV. * 4b2. If it fails for 3 times, the red LED of the port where CCTV connected blinks. | | | | |

#### Review CCTV data

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.5.2.2 | Feature Number | 3.5 | Frequency of Use | Often |
| Created date | 4/25/2015 | Author | Seokju Hong | Owner | Seokju Hong |
| Updated date | 4/25/2015 | Updated by | Seokju Hong | Revision # | 0 |
| Priority | High | | | | |
| Primary actor | SafeHome system, user | | | | |
| Title | Review CCTV data | | | | |
| Preconditions | CCTV surveillance system is activated. | | | | |
| Postconditions |  | | | | |
| Main success scenario | 1. User pushes “review” button on the SafeHome Box 2. User input administrative password to the SafeHome Box. 3. The SafeHome asks user what camera data user will review. 4. User inputs camera number and date/time range. 5. The SafeHome box replays CCTV data recorded in the input range. | | | | |
| Exceptions | 2a. Password does not match for 5 times   * 2a1. Terminate review system and lock review/retrieve function for 30 minutes.   4a. Camera ID is not applicable   * 4a1. Print error message “Camera ID is not applicable.”   4b. Date/time range is not available   * 4b1. Print error message “Datetime range is not available.” | | | | |

#### Retrieve CCTV data

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.5.2.3 | Feature Number | 3.5 | Frequency of Use | Often |
| Created date | 4/25/2015 | Author | Seokju Hong | Owner | Seokju Hong |
| Updated date | 4/25/2015 | Updated by | Seokju Hong | Revision # | 0 |
| Priority | Middle | | | | |
| Primary actor | SafeHome system, user | | | | |
| Title | Retrieve CCTV data | | | | |
| Preconditions | CCTV surveillance system is activated. | | | | |
| Postconditions |  | | | | |
| Main success scenario | 1. User pushes “retrieve” button on the SafeHome Box. 2. User connects USB memory to the SafeHome Box. 3. User input administrative password to the SafeHome Box. 4. The SafeHome asks user what camera data user will retrieve. 5. User inputs camera number and date/time range. 6. The SafeHome box copies CCTV data recorded in the input range. | | | | |
| Exceptions | 3a. Password does not match for 5 times   * 3a1. Terminate review system and lock review/retrieve for 30 minutes.   5a. Camera ID is not applicable   * 5a1. Print error message “Camera ID is not applicable.” and go back to step 5.   5b. Date/time range is not available   * 5b1. Print error message “Datetime range is not available.” and go back to step 5.   6a. Available space in the USB memory is not enough   * 6a1. Print error message “Not enough spaces in the memory” and go back to step 5. | | | | |

## Web-based monitoring dashboard system

### 3.6.1. General description

The SafeHome system serves not only emergency action services, but also system overview dashboard services. It will provide overall statistics of measured data, real-time CCTV data, summary of current status, and many more information to let users monitor their home. It is considered that web-service has the highest accessibility. Because, to use web-based application, what user need is just a web-browser, regardless of the platform. Therefore, this service will be implemented as a web-based services.

### Use cases

#### Login

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.6.2.1 | Feature Number | 3.6 | Frequency of Use | Normal |
| Created date | 4/26/2015 | Author | Seokju Hong | Owner | Seokju Hong |
| Updated date | 4/26/2015 | Updated by | Seokju Hong | Revision # | 0 |
| Priority | High | | | | |
| Primary actor | SafeHome system, user | | | | |
| Title | Login | | | | |
| Preconditions | SafeHome system is online. | | | | |
| Postconditions | User logged in to the SafeHome dashboard system. | | | | |
| Main success scenario | 1. User connects to the web page of the SafeHome system and enters his/her username and password 2. If username and password matches, login succeeds. | | | | |
| Exceptions | 2a. Username is not available or username and password does not match.   * 2a1. Dashboard system prints error message and go back to step 1. | | | | |

#### View system status

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.6.2.2 | Feature Number | 3.6 | Frequency of Use | Normal |
| Created date | 4/26/2015 | Author | Seokju Hong | Owner | Seokju Hong |
| Updated date | 4/26/2015 | Updated by | Seokju Hong | Revision # | 0 |
| Priority | Medium | | | | |
| Primary actor | SafeHome system, user | | | | |
| Title | View system status | | | | |
| Preconditions | User has logged into the SafeHome dashboard system. | | | | |
| Postconditions | Logs are printed into the web page. | | | | |
| Main success scenario | 1. User clicks “View system status” button 2. The SafeHome system filters recent logs whose level is higher than “WARNING” level, and print it out to web page. | | | | |
| Exceptions | 2a. No such log exists.   * Print “OK :)” message instead. | | | | |

#### View real-time CCTV capture

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Use case Number | 3.6.2.3 | Feature Number | 3.6 | Frequency of Use | Normal |
| Created date | 4/26/2015 | Author | Seokju Hong | Owner | Seokju Hong |
| Updated date | 4/26/2015 | Updated by | Seokju Hong | Revision # | 0 |
| Priority | High | | | | |
| Primary actor | User | | | | |
| Title | View real-time CCTV capture | | | | |
| Preconditions | User has logged into the SafeHome dashboard system.  The SafeHome system is configured properly. | | | | |
| Postconditions | User can see what camera captures real-time. | | | | |
| Main success scenario | 1. User clicks “View CCTV camera” button on the SafeHome system. 2. User selects available CCTV. 3. User can monitor his/her room with CCTV scenes. | | | | |
| Exceptions |  | | | | |

# Non-functional Requirements

## Performance Requirements

### Network Performance Requirements

* + - 1. SafeHome box must be connected with over 10Mbps internet connection.
      2. Time difference between real-time and live CCTV capture must be less than 5 seconds.

### Storage Requirements

* + - 1. Total capacity of HDD(RAID construction case included) of the SafeHome box must be at least 2TB capacity to keep CCTV data
      2. To prevent system hard disk drive corruption, RAID1 system must be constructed to the SafeHome box. And, the SafeHome box must have hot swap bay to deal with system HDD corruption.

### Memory/Architecture Requirements

* + - 1. For stability of web service and database operations, at least 4GB memory is needed.
      2. Considering upgrade of the SafeHome Box, the architecture of the CPU used in the SafeHome Box must be 64bit.

### Design/Physical Factor Requirements

* + - 1. SafeHome has its own chargeable battery which can make the SafeHome box run for 1~2 days even after power outage happens.
      2. The chargeable battery in the SafeHome Box is charged when the SafeHome Box is connected to the power outlet properly.
      3. The SafeHome Box must operates without its internal chargeable battery when it is connected to the power outlet properly.
      4. SafeHome console is expected to be durable even with free falling with 2 meter height.

## Process Requirements

### Standard Requirements

* + - 1. Platform constraints
         1. The SafeHome system runs over the environment which can works with JRE(Java Runtime Environment) properly.
         2. The SafeHome dashboard web service follows w3c web standards.
         3. The SafeHome dashboard web service must handle secure clients. SafeHome must not serve dashboard application if client uses insecure web browser(i.e. Internet Explorer 6.0)
      2. Modeling convention constraints
         1. UML 2.0 is supposed to be used as a modeling tool.
      3. Repository constraints
         1. Every work progress must be saved in company’s private git repositories, and related resources must be saved in company’s private svn server.
      4. Unit test constraints
         1. Unit test must be performed every day, at midnight.
      5. Code convention constraints
         1. Every JAVA codes must follow Google’s JAVA coding convention.

### Management Requirements

* + - 1. Record meetings in Google Docs
         1. All of the meeting is recorded in Google docs
         2. The meeting log should include the following

The names of the participants

Meeting time

Issues discussed

Action items for each participant

Confirmation of the log by every participant

Explicit references to the other development doc

Next meeting Schedule

* + - 1. Communications
         1. The communications between the participants include but not limited to

Google Docs

Kakaotalk

Facebook message

Offline conversations

## Software Quality Requirements

* + 1. Every System Features must be implemented
       1. Since every system features have high priority and is essential feature, they must be implemented.
    2. Software should be reviewed by third party
       1. The working software should be reviewed by third party. The third party includes but not limited to
          1. Professor
          2. Teaching Assistants
          3. Other project members
          4. Friends

## Security Requirements

### Access Permission

* + - 1. The permission should be only granted to the user and/or the family members of the user
      2. The permission can be granted conditionally or function by function depending on the user. For example, the user can grant permission for some feature to his/her child and not grant permission for other features.

### Privacy

* + - 1. The SafeHome device does not collect any privacy-related data from the user.
      2. The SafeHome should not let third party to gather the private data of the user.

# 

# APPENDIX

# Change Log

|  |  |  |  |
| --- | --- | --- | --- |
| **Date** | **Source** | **Author** | **Change** |
| 2015/04/22 | Initial Document creation | Young Seok Kim, Seokju Hong | Initial template development |
| 2015/04/24 | Distributed work 1 | Seokju Hong | Added distributed works |
| 2015/04/25 | Distributed work 2 | Young Seok Kim | Added distributed works |
| 2015/04/26 | Merging and polishing | Young Seok Kim | Merging both works and editing |
| 2015/04/26 | APPENDIX | Young Seok Kim | Added Change log, Glossary, Authorship |
| 2015/05/04 | Arm, disarm, alarm, etc… | Young Seok Kim, Seokju Hong | Added missing requirements |
| 2015/05/20 | Floor plan, etc… | Young Seok Kim, Seokju Hong | Added missing requirements |
| 2015/05/27 | Floor plan, recording, retrieval service, etc… | Young Seok Kim | Removed some requirements to reduced the scope of project. |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

# Glossary

1. **User**

User refers to the customers who use the SafeHome system. Similar terms would be customers, someone, or they, etc…

1. **Device**

Device refers to the SafeHome system device where the user can interact with

1. **Company**

Company refers to the SafeHome design company which sells SafeHome product

1. **SafeHome**

SafeHome can refer to the product or system or device. Unless specified, the default is referring to the SafeHome system.

# Authorship

**Seokju Hong**

* Introduction
  + Purpose, Intended Audience and Reading suggestions, Scope, Outstanding Issues
* System Features
  + 3.1, 3.5, 3.6
* Non-functional requirements
  + 4.1, 4.2.1

**Young Seok Kim**

* Introduction
  + References
* System Features
  + 3.2, 3.3, 3.4
* Non-functional requirements
  + 4.2.2, 4.3, 4.4
* Appendix
  + Change log, Glossary, Authorship
* Reviewing and Editing (including Seokju’s part and Young Seok’s part)

**Both**

* Assumptions